{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"Kalkulačka pre škárovacie hmoty"]
[]
[null,"Tu môžete ľahko vypočítať spotrebu škárovacie malty  "]
[null,"Jednoducho vyplňte označené polia!"]
[]
[]
[null,"Veľkosť obkladu"]
[null,"Šírka",30,"cm"]
[null,"Dĺžka",60,"cm"]
[]
[null,"Šírka škáry",3,"mm"]
[null,"Hĺbka škáry",6,"mm"]
[]
[null,"Plocha v m²",20,"m²"]
[]
[null,"Spotreba škárovacej hmoty",3.5999999999999996,"kg"]

{"sheet":"Tabelle2","index":1,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,null,"Fliesen"]
[null,null,"Breite",12,"cm"]
[null,null,"Länge",25,"cm"]
[null,null,"fugenbreite",15,"mm"]
[null,null,"fugentiefe",15,"mm"]
[null,null,"m²",33,"m"]
[]
[null,null,"Fugenmörtel",183.14999999999998,"kg"]

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}